;
; WifiDrv08Customizations.inf
;

[Version]
Signature="$WINDOWS NT$"
Class=Extension
ClassGuid={E2F84CE7-8EFA-411C-AA69-97454CA4CB57}
ExtensionId={49F7D94F-EC64-4AF0-A6AC-D2ED0BF9E672}
Provider=%Provider%
CatalogFile=WifiDrv08Customizations.cat
DriverVer   = 05/04/2020,21.90.3.2 ;DATE HAS TO BE IN FOLLOWING FORMAT MM/DD/YYYY

[Manufacturer]
%CompanyName% = DeviceExtensions, NTamd64.10.0...16299

[DeviceExtensions.NTamd64.10.0...16299]
; INF_GEN_PART_START DO NOT REMOVE THIS LINE!!! """%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL, <<<HWID>>> ; <<<HW>>>""" 
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_0000 ; HRP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_02F0 ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_06F0 ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_2526 ; THP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_2720 ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_2723 ; CCP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_2726 ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_30DC ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_31DC ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_34F0 ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_3DF0 ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_43F0 ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_4DF0 ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_9DF0 ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_A0F0 ; JFP
%ExtensionDescription% = CUSTOMIZATIN_EXTENSION_DDINSTALL_08, PCI\VEN_8086&DEV_A370 ; JFP
; INF_GEN_PART_END DO NOT REMOVE THIS LINE!!! 

[CUSTOMIZATIN_EXTENSION_DDINSTALL_08]
OptionDesc = %ExtensionDescription%
AddReg = Reg_Common_08


; ************************************************************************************************
; WARNING - Don't Enable this feature unless you are targeting a platform that is configured to support D3cold and was validated for it, it may Impact and harm unsupported Platforms with unpredictable behavior !!
;
; Description:      Supported D3 Hot Cold Transition. D3cold is the lowest-powered sub-state of D3. 
;                   Moving idle devices to the D3cold sub-state can reduce power consumption and extend 
;                   platform battery operation.    
; Applicability:    
; Supported HWs:    Harrison Peak, Cyclone Peak ,Jefferson Peak, Thunder Peak
; Supported OS:     Windows 10 
; Enablement:       uncomment (remove ';') from  'CUSTOMIZATIN_EXTENSION_DDINSTALL.HW' section 
;                   and the fields of this section 'Include' and 'Needs' - between START and END below
; -----------------------------------------------------------------------------------------------
; START OF SECTION TO UNCOMMENT
;[CUSTOMIZATIN_EXTENSION_DDINSTALL.HW]
;Include = machine.inf
;Needs = PciD3ColdSupported.HW
; END OF SECTION TO UNCOMMENT


[Reg_Common_08]

; ***********************************************************************************************
; Description:             DCR 133 - allow PC OEMs to set ETSI 5.8GHz SRD in Passive/Disabled
;                    ESTI SRD Channels: 149, 153, 157, 161, 165
; Applicability:    Registry key exist (DisableSRDActiveChannels) and current Geo Profile = Geo 4
; Supported HWs:    Harrison Peak, Jefferson Peak, Thunder Peak
; Supported OS:     Windows 10
; ------------------------------------------------------------------------------------------------
;               Value    Description                         Is Default
;               0        ETSI 5.8GHz SRD active scan         yes
;               1        ETSI 5.8GHz SRD passive scan        no
;               2        ETSI 5.8GHz SRD disabled            no
; ------------------------------------------------------------------------------------------------

HKR,,DisableSRDActiveChannels,0x00010001,0

; ***********************************************************************************************

; ***********************************************************************************************

; Description:      DCR-177 - Support Wi-Fi/LAA antenna switch.
;                            Special industrial design constraints which prevent from adding dedicated LAA antennas.
;                            The control of the antenna will be from Wi-Fi,
;                            to give Wi-Fi priority and avoid issues where Wi-Fi may transmit without owning the antenna.
;
;                            Note: enablement of this  feature depended on the HW of the LAA/Wi-Fi antenna switch and CPL approval
;                                     all other platforms without the LAA switcher the feature should be in disabled mode(the default).
; Applicability:    Registry key ‘LaaAntSwitchSupport’
; Supported HWs:            Cyclone Peak, Thunder Peak,
; Supported OS:                Windows 10 DT/WCOS
; ------------------------------------------------------------------------------------------------
;               Value    Description                                                  Is Default
;               0        LLA_ANT_SWITCH_NOT_SUPPORTED               yes
;               1        LLA_ANT_SWITCH_ENABLE_ON_HB   no
; ------------------------------------------------------------------------------------------------

HKR,, LaaAntSwitchSupport,0x00010001,0

; ***********************************************************************************************

[DestinationDirs]
DefaultDestDir=12 ; DIRID_DRIVERS

[SourceDisksFiles]

[SourceDisksNames]
1 = %DiskName%,,,""

[Strings]
Provider="Intel"
ExtensionDescription="Intel(R) Wireless Driver Customization"
CompanyName="Intel Corporation"
DiskName = "Intel(R) Wireless Driver Customization Install Disk"

